2019 Compact Class Demolition Derby Rules...  
1. All drivers and pit persons will sign a waiver releasing all officials of any responsibility and liability in  
2. If a driver or pit person is under the age of 18, they must have a waiver of liability signed by a parent or legal guardian. NO ONE UNDER THE AGE OF 12 ALLOWED IN THE PITS!  
3. All vehicles must pass tech inspection after being registered to receive qualifying stick. (NO REFUND  
4. Front wheel drive only. No V-8s.Max 6-cylinder engine. No rear wheel drive compact cars.  
5. Vehicle must have a working seat belt. Belt must be bolted to the floor or frame.  
6. All mirrors, loose chrome, headlights, taillights and exterior door handles must be removed.  
7. Remove all windows. All broken glass must be removed.  
8. Back seats and all carpet and fire hazards must be removed. Trunk must be empty.  
9. Engine may be interchanged from any make – must be in stock location, no cutting out of firewall. NO cradles, carb protectors, or distributor protectors allowed.  
10. Vehicles must be numbered (18” in height) on both front doors and roof. Mandatory 18”X18” roof # sign.  
11. DOORS: Drivers door maybe welded solid all other doors may be welded using 3x3 ¼ thick plates in 4 locations You also may use chain our cable ¾ thick max in 4 locations  
12. HOOD: you may use 1’’ threaded rod in 4 locations welded to the side of the frame or to the top of the frame DO NOT go thru the frame OUR you may use chain our cable ¾ max up to 4 locations you may crease the trunk you must have a 4x4 inspection hole hood must have an opening of 7x7 just in case if there’s a fire  
13. Battery to be moved into passenger compartment. Battery must be ratchet strapped to floor in a minimum of 2 locations or securely bolted in a minimum of 4 locations. Battery must be boxed in wood or metal. Sides of box must be as tall as battery case. Must have some type of battery cover. No rubber tarp straps securing battery in place. (may be used on battery cover)  
16. CAGE:A support bar behind driver’s seat is allowed. A steering support is also allowed. Maximum 4” diameter round or square pipe behind seat. 4” max diameter for steering support. Max 8”X8” flat plate on ends of pipe no more than 3/8” thick – No galvanized pipe allowed. No other cross members to strengthen the frame. No bars forward or backward to the frame or floor. Halo bar allowed, may be welded to rear seat support bar on top or side of bar. Halo may not extend to floor board, you may bolt you halo to the roof ½ bolts in 3 locations do not weld the halo to the roof  
17. Two windshield bar and one rear window safety bar allowed, 3” max diameter. May be bolted in place or welded, may not exceed onto roof or deck area by more than 6”.  
18. BUMPERS you may run any mass produced bumper no stuffing or homemade bumpers bumper end must be open for inspection bumpers can be welded directly to the frame bumper bracket must remain stock and must remain in their stock location  
19. FRAMES: must remain stock there should be no welding on the frame other than what’s stated in the rules body bolts must remain stock  
20. Suspensions must remain stock no solid suspension is not allowed  
21. TIRES-you may run tire of your choice noting bigger the 16inch all wheel weights must be removed   
22. Stock gas tank must be moved into the vehicle. Fuel cells are highly recommended, stuck tank may be used if securely fastened and all fuel pump and fuel lines are covered.   
23. Transmission coolers allowed – high temp hose and steel-doubled clamped – All hoses must be covered.  
28. Vehicle must have minimum of two working brakes at time of inspection.  
\*\*IF A CUTTING TORCH IS BROUGHT INTO THE PITS  
YOU MUST HAVE A FIRE EXTINGUISHER ON SITE AS WELL\*\*  
We reserve the right to modify any rules as needed.